{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["车身涂装"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"车身涂装","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"merged":[[0,0,0,7],[11,0,11,6]],"flags":["formulas_cached_only"]}
["济南理工学校汽车工程系车身涂装技能大赛、教学实训耗材采购"]
["序号","名称","品牌型号","参数","单位","数量","参考单价","参考总价"]
[1,"万能原子灰（合金腻子）","Nexa Autocolor  P551-1052","2公斤一桶，符合2019年车身涂装项目国赛标准使用","桶",4,null,0]
[2,"稀料","一般品牌","300mm*650mm60L符合国家安全标准 对人体无伤害 可再回收利用","桶",1,null,0]
[3,"圆形砂纸","费斯托","圆形，直径150mm，48孔，P320、P400（100张每盒），符合2019年车身涂装项目国赛标准使用","盒",2,null,0]
[4,"2K高固固化剂","Nexa Autocolor  P210-8430","2K高固固化剂，2.5升一桶，符合2019年车身涂装项目国赛标准使用","桶",1,null,0]
[5,"闪电清漆","Nexa Autocolor  P190-6208  P210-6863","闪电清漆5升一桶，符合2019年车身涂装项目国赛标准使用","桶",1,null,0]
[6,"2K高固含量稀释剂","Nexa Autocolor  P852-1689","2K高固含量稀释剂，2.5升一桶  （超快干），符合2019年车身涂装项目国赛标准使用","桶",1,null,0]
[7,"环氧底漆","Nexa Autocolor  P565-895","超快干无铬环氧底漆，1L一桶，用于裸漏金属的施涂，符合2019年车身涂装项目国赛标准使用","桶",1,null,0]
[8,"高固含量厚膜底漆（灰色）","Nexa Autocolor  P565-510","高固含量厚膜底漆，3.5升一桶，符合2019年车身涂装项目国赛标准使用","桶",1,null,0]
[9,"玻璃升降器更换及车门调整工作站","大赛型","三层工具车 \n品牌：强斯威；型号：C-T12；箱体尺寸 716×410×752MM；含轮尺寸 716×410×880MM；重量：20.2Kg。\n128件套综合性工具组套\n品牌：强斯威，型号：S04H524128S，\n12件6.3MM系列6件公制套筒，5件6.3MM系列六角公制长套筒\n6件6.3MM系列六角旋具套筒，5件6.3MM系列花型旋具套筒\n1件6.3MM系列万向接头，2件6.3MM系列转向接杆\n1件6.3MM系列滑行杆，1件6.3MM些列转向手柄\n1件6.3MM系列专业快速脱落棘轮扳手，1件6.3MM系列接杆\n8件12.5MM系列六角公制套筒，7件12.5MM系列六角公制长套筒\n3件12.5MM系列六角旋具套筒，2件12.5MM系列磁性火花塞套筒\n1件12.5MM系列转向接杆，1件12.5MM系列滑行杆，1件12.5MM些列万向接头\n2件12.5MM系列接杆，1件12.5MM系列转向手柄，19件公制两用扳手\n5件公制油管扳手，9件公制内六角扳手，7件花型扳手，5件套样冲\n1件10\"收泵钳，1件6\"斜口钳，1件7\"钢丝钳，1件磁性棒\n1件木柄钳工锤，6件螺丝批，1件吹气盒  \n塑钢撬棒组\n品牌：强斯威，型号：AB010026S\nA/B/C/D/E五种楔型撬棒，可方便移除车内饰板上的扣子\n可用于撬拉拽等动作，避免损伤内饰板","套",1,null,0]
["合计",{"$nulls":6},0]